# DataMan DataMan 8600 Base Station Specifications

Specification | DMA-IBASE-01
--- | ---
Weight | 328 g
Operating Temperature | 0 ºC — 40 ºC (32 ºF — 104 ºF)
Storage Temperature | -40 ºC — 60 ºC (-40 ºF — 140 ºF)
Maximum Humidity | 95% (non-condensing)
Power Supply Requirements | 24 V +- 10%, 13 W maximum LPS or NEC class 2 power supply, or PoE class 3 (connect only to PoE networks without routing to the outside plant)
Protection |