# IMAGE.SERVER-FINGERPRINT

Allows readers to verify the SFTP server identity. Ask your SFTP server admin for the fingerprint hash and provide the hash in this command. If the entry is empty, the reader does not check the server identity. The reader only checks the identity if the server type is SFTP.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
hash | string | Server-hash | No fingerprint check happened: SFTP server hash is empty. Fingerprint check happened: the server fingerprint hash starts with "md5:" or "sha1:" or "sha256:".

## Platforms

DM50, DM60, DM70, DM80, DM260, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050, DM8600

## Notes

Version: 25.4