# LIGHT.COLOR-CHANNELS

Sets the color of the illumination during acquisition or returns the current color. You can set only one of the arguments for the SET LIGHT.COLOR-CHANNELS ON/OFF ON/OFF ON/OFF ON/OFF to ON. For example, SET LIGHT.COLOR-CHANNELS ON OFF OFF OFF enables red.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
red | bool | [ON|OFF] | Enable state for the color channels on a multicolor illumination. The number of available channels is hardware dependent.
green | bool | [ON|OFF] | Enable state for the color channels on a multicolor illumination. The number of available channels is hardware dependent.
blue | bool | [ON|OFF] | Enable state for the color channels on a multicolor illumination. The number of available channels is hardware dependent.
white | bool | [ON|OFF] | Enable state for the color channels on a multicolor illumination. The number of available channels is hardware dependent.

## Platforms

DM282 with HPIT.

## Notes

Version: 6.3.4