# ENCODER.VIRTUAL-RESOLUTION

Sets or gets the resolution of the virtual encoder. The virtual encoder allows you to use a distance per tick that is different from that of the attached physical encoder.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
resolution | int | [1-1000000] | Resolution in micrometers

## Platforms

Fixed-mount readers with virtual encoder support

## Notes

Version: 25.4