# LIGHT.HIGH-FREQUENCY-ALWAYS

Enables High Frequency Light in Continuous trigger mode even if no trigger is active. After duration seconds the High Frequency Light is turned off. If the duration is 0 the light is never turned off.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
enable |  | [ON|OFF] | enable/disable
seconds | int | 0-86400 | auto off duration

## Platforms

DM50, DM60, DM70, DM300, DM360, DM370, DM470, DM503

## Notes

Version: 5.2.0