# CAMERA.EXPOSURE-US

Camera Parameters where exposure is in microseconds. The argument 'exposure' and 'gain' has no effect if 'auto' is ON and 'target' has no effect at all.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
auto |  | [ON|OFF] | ON: Automatic
target | int | [0-255] | target pixel value
exposure | int | [50-25000] |
gain | int | [0-60] | camera gain

## Platforms

MX-1000 and DM8000.

## Notes

Version: 5.5.0