# PCM.METRIC-PARM-OVERALL

Use the the metric grading result for calculating the overall result if enabled (e.g. AIM-DPM → Symbol Contrast → Use for Overall Calculation = ON) Not all metrics are available for each standard: AIM-DPM (0, 1, 2, 3, 4, 5, 6, 8), ISO-IEC 15415 (0, 1, 3, 4, 5, 6, 7), ANSI-ISO-IEC 15416 (1, 4, 8, 9, 22, 23, 24, 25), 1D readability (0, 2, 8, 9, 10, 11), DotCode (0, 1, 2, 3, 6, 8)

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
type |  | [0-5] | 0: AIM-DPM
type |  | [0-27] | 0: Symbol Contrast
state |  | [ON|OFF] | ON: use for overall calculation

## Platforms

Ethernet readers.

## Notes

Version: 5.7.0