# HPIT.OUTPUT-CONFIG-CUSTOM-INDICATOR

Enable/Disable the use of the right HPIT indicator functionality with a given time length. As a default, none of the outputs is enabled.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
OUTPUT_NUMBER | int | [0-27] | 0 = Good read
state | bool |  |
TIME_LENGTH_US | int | [0 - 20000] | microseconds

## Platforms

DM370, DM470.

## Notes

Version: 6.1.7