View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is ISO Validation?

The ISO Validation feature is used to determine if a data string is correctly encoded according ISO 15434 syntax or ISO 15434 plus ISO 15418.

ISO 15434 confirms if the data string is encoded with the correct syntax which includes the evaluation of the ‘non-printable' ASCII characters in the string such as the message header, record separator, format code (For AI, DI or TEIs), group separators and end of transmission character.

ISO 15418 confirms if the data string is encoded with the correct Data Qualifiers for each Data Element. Depending on whether a manufacturer is using a AI, DI or TEI format, each Data Element (Manufacturer's EIN code, Part Number and Serial Number) is preceded by a specific code or ‘Data Qualifier'.

Note: This option is not available on all readers.

Note: This option also allows Text Element Identifiers as defined in the ATA CSDD specification.

Note: default,DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM470, DM503,DM7500,DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500