# COM.USB-HID-EJECT-BUTTON

Enables sending an eject button over Bluetooth HID. With this command, iPhone users can bring up the virtual keyboard on their devices, when it is connected to a DM8700 reader through Bluetooth. If you pull the trigger button twice under 0.75 seconds, the virtual keyboard pops up on the connected iOS device. By default, the command is disabled.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
state | bool | [ON|OFF] | enable/disable

## Platforms

DM8700 Bluetooth readers

## Notes

Version: 6.2.7