# CAMERA.EXPOSURE-US

Camera Parameters where exposure is in microseconds. The argument 'exposure' and 'gain' has no effect if 'auto' is ON and 'target' has no effect at all. The 4th parameter (GAIN) has no effect on DM370 and DM470.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
auto |  | [ON|OFF] | ON: Automatic OFF: Manual
target | int | [0-255] | target pixel value
exposure | int | [5-1000] | DM300 and DM302 internal illumination DM303 internal illumination with external or no illumination
gain | int | [0-106] | camera gain

## Platforms

DM280, DM300, DM360, DM370, DM470, DM8600

## Notes

Version: 5.5.0