# PCM.USE-CUSTOM-THRESHOLDS

Enable or disable regrading of metric results by using the custom thresholds.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
type |  | [0-5] | 0: AIM-DPM 1: ISO-IEC 15415 2: ANSI-ISO-IEC 15416 3: SemiT10 4: 1D readability 5: DotCode Readybility
state |  | [ON|OFF] | ON: do regrading OFF: keep current result

## Platforms

Ethernet readers.

## Notes

Version: 5.7.0