View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How does trigger delay work in Multi-Reader Sync Mode?

Primary Reader and Secondary Readers are normally triggered at the same time, however, a trigger delay can be set for the Primary reader and each Secondary reader in the group. The total trigger delay time for the Primary reader will simply be the trigger delay time set on the Primary reader. The total trigger delay time for the Secondary reader will be the Primary reader trigger delay time + Secondary reader trigger delay time.

Note: DM060,DM070,DM260,DM300,DM360, DM370, DM470, DM503