# HPIT.RANGE-DETECTION-BOUNDED-FOCUS-ENABLED

Enables/Disables the clamp focus functionality. When active, if the target is out of range, the liquid lens focuses at a distance the user defines (default 500 mm).

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
state |  | [ON|OFF] | enable/disable

## Platforms

DM370, DM470 with HPIT.

## Notes

Version: 6.1.8