# HPIT.AUTOFOCUS-CONTROL-ENABLE

Enables/Disables the auto-focus (ToF guided focus) functionality. During auto-focus, all manual changes of focus are disabled and the height sensor measurement is used as a reference for the focus distance. For minimum target sizes please refer to the manual.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
state |  | [ON|OFF] | enable/disable

## Platforms

DM370, DM470 with HPIT.

## Notes

Version: 6.1.6 SR2