# TRIGGER.TYPE

Trigger Type. The camera API should return the current trigger type value.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
type | enum | [0-5] | 0: Single (external) 1: Presentation (internal) 2: Manual (button) 3: Burst (external) 4: Self (internal) 5: Continuous (external)

## Platforms

DM8000 support only Presentation and Manual trigger types. DM280. MX-1000, MX-1502 and Mobile support only Manual and Continuous trigger types.

## Notes

Version: 3.0.0