View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is GS1 Validation?

GS1 validation allows you to verify the syntax and semantics of symbols against the GS1 specification. The reader can validate the encoded data against a configurable string of identifiers. All application identifiers are supported.

By default, the reader validates the incoming symbol against the European Federation of Pharmaceutical Industries and Associations (EFPIA) format string, for example:

<AI(01)><AI(10)><AI(17)><AI(21)>

Using GS1 validation, you can configure what the reader transmits when the data in a symbol does not pass verification, including a carriage return and line feed. The Detailed Results pane will display a PASS or FAIL for each symbol and list each application identifier in the symbol along with its accompanying data element.

Note: default,DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM470, DM503,DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500