View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What error does an orange arrow indicate in Symbol Diagnostics?

An orange arrow indicates that Start or Stop pattern was not found. The region designated by the arrow failed to decode. Reasons for failure are as follows (please check the corresponding Tech Note for detailed images that illustrate each case):

- The Start or Stop pattern is clipped/damaged

- The code is clipped (due to image boundary or by an object blocking the code)

- Image quality degradation (often, but not always, caused by light quality)

- Warping and folding of barcode labels

Note: Note: Symbol Diagnostics is a feature that is activated exclusively by feature key.

Note: DM070,DM150,DM260,DM300,DM360, DM370,DM280, DM470, DM503