View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is Distance-Based Triggering?

Distance-Based Triggering means that a trigger sequence is initiated if the reader’s distance sensor records an object within a preset distance range. For example, if the range is set to 500 mm -1000 mm and the distance sensor records an object at 600 mm, the trigger sequence starts, while an object recorded at 400 mm stops or does not initiate the trigger sequence.

Note: DM370,DM280,DM470