View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What data does Performance Overview collect and display?

Performance Overview can display Read Rate, Reads per minute, and NoReads per minute in a real-time graph, depending on the setting in the top left under Displaying. The Last [time interval] buttons on the top row are clickable, and the active is outlined orange. You can use the buttons to set the interval that Performance Overview uses.

You need to trigger the monitored device for data to be displayed on the graph.

You can set up a warning line to appear on the graphs under Configuration > Display Settings. Checking the box makes the warning line to display on each graph. Chart Type determines what kind of line is displayed, while ReadRate Reference Line Value (%) is the percentage where the line is drawn on the graphs.

Note: DM060,DM260,DM300,DM360,DM503, DM370,DM280, DM470, RTM_Lean