View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the What Images to Buffer for a Result option?

You can choose what images to buffer for a result.

Select All for the reader to store every acquired image up until the maximum number of images per result or the maximum number of images have been reached. Select Auto for the reader to do intelligent image buffering (requires the IntImageBuffer feature key). Select Same as result for the reader to store only images with a found code for a good read. Select First for the reader to store only the first image in the trigger cycle of the specified trigger mode. Select Last for the reader to store only the last image in the trigger cycle of the specified trigger mode. Select First and Last for the reader to store both the first and the last images in the trigger cycle of the specified trigger mode.

Note: default,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370,DM280, DM470, DM503,DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500