View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do I adjust the image exposure?

In the Exposure group, Automatic Exposure automatically determines the best settings for a desirable level of brightness in each image. You can use Maximum exposure settings as necessary for your production environment. Alternatively, select Manual Exposure and set a precise exposure time in microseconds.

With Manual Exposure, you can click Optimize Brightness on the Result History pane to generate a fixed value for the exposure setting limited by the Maximum exposure value. The Gain slider (below the image view area) indicates the target's pixel brightness.

Note: DM8050,DM8070