# WIFI.ENC-METHOD

Sets the authentication method.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
int |  | [0-5] | 0 – off 1 – WEP40 2 – WEP104 3 – TKIP 4 – AES 5 – TKIP/AES

## Platforms

DM8000;Base

## Notes

Version: 4.2.4

Copyright © 2011-2022 | Cognex Corporation | All Rights Reserved.

DMCC Reference | 2022 September 22 | Revision: 1.4.0.26