# Resolved Issues

This section describes changes and resolved issues in In-Sight 3D EasyBuilder 24.2.0.

Note: Issue numbers (Issue #) have been included (where applicable) to improve tracking of Known Issues reported via Cognex Technical Support.

##### Resolved Issues in In-Sight 3D EasyBuilder 24.2.0

Issue # | Resolved Issue
ISPROD-2677 | EditFloat minimum and maximum values did not set properly after dragging from Property sheet to Spreadsheet.
ISPROD-2987 | DetectBlobs GetPolygon() did not draw graphics.
ISPROD-5839 | ErrFree function was hidden.
ISPROD-13506 | ColorToGreyscale failed when converting using Hue.
ISPROD-13963 | Selecting Backup when updating the In-Sight L38 firmware did not work. Backup now reports progress during download.
ISPROD-14368 | Network properties of Ethernet could not be restored over USB ports.
ISPROD-15264 | Native mode command parsing did not execute commands related to cells in rows > 399.
ISPROD-15822 | The ELRead CJK Unicode exception prevented Asian character labeling.
ISPROD-16216 | The password reset failed on the In-Sight 3805C and L38 vision systems.
ISPROD-16389 | The Discrete I/O HSOUT0 setting only supported Programmed mode.
ISPROD-16404 | The Discrete I/O output delay behavior was corrected.
ISPROD-16822 | The WebHMI API did not persist startup jobs.
ISPROD-17041 | Unable to edit the PixelCount range slider.
ISPROD-17157 | Faster multiple settings change in L38. It now takes 1100ms to go online in comparison to the previous 500ms.
ISPROD-17182 | The Measure Distance tool did not show the line between two points.
ISPROD-17394 | The PropertyLinkRangeSlider did not allow editing when the max value is bound to a cell with #ERR.
ISPROD-17778 | In-Sight 3D EasyBuilder crashed when interacting with some acquisition wizard controls while configured in Japanese.
ISPROD-18060 | Scan length setting could not be updated.
ISPROD-18211 | Remove hardcoded timeout during restore.