# Image

The Image application step of the EasyBuilder allows you to define the image source and optimize the device lighting.

Section | Tool | Action
--- | --- | ---
Source | Camera | To create a job based on the direct feed from your In-Sight vision system, select Camera under Source.
Image Folder | To create a job based on a set of images stored on your hard drive, click Image Folder under Source.
Lighting | Optimize | To auto-set the exposure based on current light settings, click Optimize.There is no exposure adjustment by default.
Exposure (ms) | To increase or decrease illumination intensity, use the Exposure slider or set a value below the slider.
Light Color | To define the illumination color, select a color (WHITE, RED, GREEN, BLUE) from the Light Color dropdown menu. Note: The light color tool appears only if a Multi Torch is connected to the vision system.
Focus | Optimize | To auto-set the focus, click Optimize.There is no focus adjustment by default.
Focus Position (mm) | To adjust the focus position, use the Focus Position slider or set a value below the slider.