# Password Reset

Note: This utility can also be used to configure multiple devices at the same time. To select multiple devices on the In-Sight® Device Pane, either press Shift + Left Click on the first and last devices in the list you want to configure, or press Ctrl + Left Click to select multiple devices one after the other.

The Password Reset utility is used to reset the password of the default admin user on the selected In-Sight device(s). Use it as follows:

1. Launch In-Sight Vision Suite if it is not already running.

2. Left-click the device you want to configure on the In-Sight® Device Pane on the left. The list of Utilities applicable to the selected vision system then appears at the bottom of the window.

3. Click the Password Reset button in the list of utilities to launch the Reset Password dialog.

4. Click Reset. The utility then asks for power cycling the vision system to complete the password reset.

5. Click Reset to continue with the password reset, or click Cancel Reset to cancel the procedure and close the dialog. Once power cycling is finished, the admin user has a blank (or empty) password again.

Note:

You can only reset the password of devices that are located on your local subnet. Attempting to reset the password on a device located on a remote subnet returns a Password reset is only supported for devices on the local subnet error message.