# TransInspEdgeWidthToWorld

Applies a coordinate transform to an InspectEdgeWidth data structure.

Note: The output of any vision tool that reports in real-world coordinates cannot be used as a fixture or region input to another vision tool.
Inputs

Parameter | Description
Calib | A reference to a spreadsheet cell containing a valid Calib data structure.
InspectEdgeWidth | A reference to a spreadsheet cell containing a valid InspectEdgeWidth data structure.

Outputs

Returns | InspectEdgeWidth structure translated to real-world coordinates, or #ERR if any of the input parameters are invalid.