# Operator Interface (WebHMI) Overview

The operator interface, or WebHMI is an interface through which the operator interacts with the vision system.

You can configure what job properties and results appear on the WebHMI in your Spreadsheet or EasyBuilder job. To access the WebHMI, select your device in the In-Sight Vision Suite home page and click the Open HMI button, or navigate to <device_IP_address>/pages/hmi/ in your browser.

The WebHMI has four main components:

Number | Element | Description
1 | Main panel | Image and the image control buttons.
2 | Output panel | Job properties that you added.
3 | Settings panel | Controls of the vision system.
4 | Result Queue | Result queue panel.

## Main Panel

Number | Element | Description
1 | Zoom in | Zoom into the image.
2 | Zoom out | Zoom out from the image
3 | Fit | Fits the image to the borders of the Main panel.
4 | Fill | Fits the image into the entire Main panel.
5 | Rotate Left | Rotates the image to the left by 90 degrees.
6 | Rotate Right | Rotates the image to the right by 90 degrees.
7 | Pan On/Off | If enabled, you can adjust the image by clicking the arrows.

## Settings Panel

Number | Element | Description
1 | Hide/Unhide | Hides/Unhides Settings panel.
2 | Information | Information about the vision system.
3 | Load/Save | Loads/Saves job.
4 | Online/Offline | Switches between Online and Offline mode.
5 | Trigger | Triggers the vision system.
6 | Live Mode | Switches the live mode on or off.
7 | View Options | Switches between EasyView and Custom View.
8 | Dropdown list | Dropdown menu of the available EasyViews and Custom Views.
9 | Image/Graphics | Hides/Unhides the image or the graphics.
10 | Settings | Settings options for WebHMI. For more information, see WebHMI Settings.

## Result Queue Panel

Number | Element | Description
1 | Freeze/Continue | Freezes or continues to show an image from the filmstrip
2 | Play First | Plays first image.
3 | Play Previous | Plays previous image.
4 | Filmstrip | Shows the result images.
5 | Play Next | Plays the next image.
6 | Play Last | Plays the last image.
7 | Download | Downloads filmstrip.
8 | Clear | Clears filmstrip.