# PlotProfile3D

The PlotProfile3D function allows you to draw a 3D profile with specific settings. The constructed profile is returned in a Plot structure.

Inputs

The PlotProfile3D function has the following syntax:

PlotProfile3D(PointCloud,ExternalProfile,Name,Color,Transparency,LineDrawingThickness,Show)

Parameter | Description
PointCloud | Reference to a cell containing a point cloud. The default value is $A$0.
External Profile | Specifies a reference to a 3D profile defined in another cell.
Name | The label of the plotted structure. The configured string appears next to the structure.
Color | Specifies the color of the profile and the profile label. The default value is Lime Green.
Transparency | Specifies the transparency of the profile. The value range of the property is 0 – 100 (from no transparency to complete transparency), and the default value is 0 (meaning no transparency).
Line Drawing Thickness | Specifies the drawing line thickness for lines, edges, and wireframes.
Show | Selects the display mode.
0 (Unchecked) = Off | The structure will be hidden, except when the cell containing the function is highlighted in the spreadsheet.
1 (Checked) = On (default) | The structure will be displayed at all times.

Outputs

Returns | A Plot structure that allows you to modify the plotted 3D profile.
Results | When inserted into a cell, a ❒Plot structure is created, containing the settings of the 3D profile drawn in the point cloud when the job is Online.