# Resolved Issues

This section describes changes and resolved issues in In-Sight Spreadsheet 24.4.0.

Note: Issue numbers (Issue #) have been included (where applicable) to improve tracking of Known Issues reported via Cognex Technical Support.

##### Resolved Issues in In-Sight Spreadsheet 24.4.0

Issue # | Resolved Issue
--- | ---
ISPROD- 21615 | Fixed a memory leak in the 3D HMI when working with height color.
ISPROD-21438 | Fixed an error where the audit log always shows the auth user as admin, regardless of the user that is logged in.
ISPROD-21179 | Fixed an issue with the PlotRectangle3D function failing to produce any output.
ISPROD-21034 | Fixed an error that was causing crashes when adding the Math tool to a Group in EasyBuilder.
ISPROD-21006 | Eliminated the delay that occurs when performing an acquisition using a software trigger with an In-Sight L38 vision system.
ISPROD-21005 | Fixed an issue with hardware triggering when using encoder based acquisition in L38 vision systems. Depending on when the vision system received the trigger, it could hang the acquisition.
ISPROD-20839 | Fixed an error with the order of the colors in the color list produced by TrainExtractColor function being randomized when closing and re-opening the function property sheet.
ISPROD-20785 | Fixed an error with In-Sight L38 vision systems producing an error when triggering after optimizing the exposure in EasyBuilder.
ISPROD-20649 | Corrected the behavior of the Jump function so that the highlighted cell always shows in the top left corner of the spreadsheet.
ISPROD-20529 | Fixed an issue with the default getter functions for the ExtractColor function failing to sort the models in descending order of pixel count.
ISPROD-20478 | Fixed an issue with loading user settings that was causing crashes.
ISPROD-20477 | Fixed an issue where the WriteImage and WriteData functions cannot save files through SFTP when the file path is empty.
ISPROD-20446 | Fixed the vision system and firmware version to display correctly when using an In-Sight L38 vision system in GEV server mode.
ISPROD-20383 | Fixed an issue where the WriteImage function truncates the file name after the final period in the SVG content if the File Name string contains one or more periods. This error occurred when saving SVG files through FTP/SFTP.
ISPROD-20257 | Fixed an issue with the Format String configuration accepting further arguments after exceeding the maximum expression length, and silently dropping any arguments above the maximum threshold after closing the window.
ISPROD-20212 | Fixed an issue with the FormatString producing an error when using a double quote mark in a label.
ISPROD-19882 | Fixed an issue with Spreadsheet cells not being able to reference EditMultiGraphics cells.
ISPROD-19774 | Fixed an issue with the WriteImage function causing crashes when using a reduced ROI and Render on Image settings.
ISPROD-19215 | Fixed an issue with the WriteImage function not rendering graphics when using In-Sight L38 vision systems.
ISPROD-18827 | Fixed an issue with users not being able to delete saved images in sub-directories.
ISPROD-18601 | Fixed an issue with jobs not loading on the emulator when they contain TrainPatMaxRedLine functions.
ISPROD-18497 | Fixed an issue with some triggers silently dropping and not returning acquisitions when using In-Sight 3800 vision systems, which was causing misalignment between inspection IDs and acquisition IDs.
ISPROD-18237 | Fixed an issue with the Math tool in EasyBuilder causing null reference exception errors when changing app steps while modifying cells.
ISPROD-18112 | Fixed an issue with the WriteImage function truncating the image href after a period in SVG files when saving through FTP.
ISPROD-16738 | Fixed an issue with high gain settings on In-Sight 3800 vision systems producing images with inconsistent brightness depending on the trigger interval.
ISPROD-14110 | Fixed an issue with the Blob tool not using calibration data.
N/A | Fixed an issue where editing the acquisition settings for an L38 vision system through the ApplyAcquisitionSettings3D function did not update the configuration correctly. The vision system used the Along XY setting when you selected Along X for the Median Filter parameter, and used the opposite mode to your selection for Gap Filling Mode and Spike Hole Filling Mode.