# $ Functions: System

    $System.GetSysReport()
Returns | SysReport class member defined with the related tags.
Arguments | N/A
Description | Returns the system information specified with the following tags: HostName: String, returning the host name of the In-Sight 3D vision system. IPAddress: String, returning the IP address of the vision system. MacAddress: String, returning the MAC ID of the vision system. Model: String, returning the model name of the vision system. SerialNumber: String, returning the serial number of the vision system. Version: String, returning the version of the vision system firmware. ヒント : The system information available with this $ function can also be checked with the System Info button of In-Sight Vision Suite. Refer to the System Info topic of the In-Sight Vision Suite Help for more information.
Example | The below example is a set of system checks:
    $HostName = $System.GetSysReport().HostName;
    $IP_Address = $System.GetSysReport().IPAddress;
    $FWversion = $System.GetSysReport().Version;
    $MAC_address = $System.GetSysReport().MacAddress;
    $SerialNumber = $System.GetSysReport().SerialNumber;
    $Model = $System.GetSysReport().Model;
You can then call the value of these checks, for example, in WebPage Labels by setting their Text property accordingly with the Expression Builder.

    $System.GetUptimeMilliseconds()
Returns | Double, indicating controller uptime in milliseconds (but with microsecond accuracy, hence the fract-digits).
Arguments | N/A
Description | Returns the uptime of the vision system in milliseconds (but with microsecond accuracy).

    $System.Log.Write(message : String, logLevel : Integer)
Returns | N/A
Arguments | message : String, specifying the log message to record. logLevel : Integer, specifying the severity of the log message. Its value must be between 0-3, corresponding to the following severity levels: 0: Verbose 1: Info 2: Warning 3: Error 注 : Log messages set to Verbose severity (that is, 0) will not be shown in the IDE system log.
Description | Records a log message on the vision system, which is read and displayed by the output window dialog of In-Sight. The recorded log - presuming that the IDE is running - will be recorded to the system log output file as well, available in the following location by default: \Documents\In-Sight Vision Suite\Logs