# Known Issues

The following known issues have been identified in this release:

Note: Issue numbers (Issue #) have been included (where applicable) to improve tracking of Known Issues reported via Cognex Technical Support.

Issue # | Known Issue
--- | ---
ISPROD-151 | Undo of tool deletion with certain property links might not restore links in EasyBuilder Communications
ISPROD-1330 | When you fixture a pattern tool to another pattern tool, the tool location moves properly with the fixture. However, the angle does not. More specifically, the angle range appears to reference the main image and not the fixture.
ISPROD-2160 | Emoji or Unicode password characters are not supported, but are occasionally allowed.
ISPROD-2351 | With the Windows setting Automatically hide the taskbar in desktop mode, if you run In-Sight EasyBuilder with a maximized window, you cannot access the taskbar.
ISPROD-3869 | WriteImage does not create subfolders on the FTP server and fails to transfer if the folder does not already exist. To avoid this, ensure that the directories exist before attempting to write to them via FTP.
ISPROD-4705 | A .bmp image saved from one In-Sight 2800 sensor is unable to open on another In-Sight 2800 camera.
ISPROD-5485 | Attempting to connect to both instances of a dual ethernet vision system by selecting both and then clicking on a connect option in ISVS reboots the sensor. The sensor needs to be physically power cycled.
ISPROD-6355 | Incorrect data size is listed for bit Data Type in the Outputs list.
ISPROD-6536 | A momentary network interruption disrupts emulator when working with ViDi EL Tools and the cloud dongle.
ISPROD-6605 | The EasyBuilder Pattern tool PlotRegion fails when CompositeRegion is a circle.
ISPROD-7521 | Issues with the image border on the HDR+.
ISPROD-8923 | A job with many Edge Learning tools fails to load due to a UI timeout.
ISPROD-8936 | The EasyBuilder Pixel Tool Input Composite Region from Math tool does not use angle correctly.
ISPROD-9046 | Restore fails when .bak has large jobx files.
ISPROD-9189 | Switching views in WebHMI makes graphics disappear.
ISPROD-9256 | The Offset in Acquisition Settings changes in multiples of 8.
ISPROD-10220 | Exposure default value is loaded from the job if the saved value is above the maximum exposure.
ISPROD-10723 | Restore or Backup fails when files have spaces in their names.
ISPROD-11032 | 1D Symbology Result Regions are sometimes drawn with slightly incorrect rotations when many results are returned.
ISPROD-11459 | Live mode does not work with partial acquisition settings.
ISPROD-11660 | Not all EasyBuilder Inspect tool ROIs are highlighted on mouse hover.
ISPROD-12033 | The EasyBuilder Classify Edit Class view sometimes does not close when a new job is started.
ISPROD-12124 | In-Sight Emulator fails to start if MyDocuments is a network drive.
ISPROD-12641 | Even if the Trigger Input Line in Acquisition Settings is disabled, the system accepts a trigger at Discrete Input0.
ISPROD-13727 | Cannot start or stop the filmstrip recording while online.
ISPROD-13773 | The Calibrate Grid utility generates incorrect image with 1 mm spacing.
ISPROD-13864 | The UI connection sometimes disconnects from the vision system if a job takes too long to load.
ISPROD-13957 | With the new Orion lens, the EasyBuilder autofocus can take longer and the UI appears frozen for 5 seconds.
ISPROD-14167 | The SortPatterns tool in FindPatMaxPatterns can crash the In-Sight EasyBuilder.
ISPROD-14338 | The Backup/Restore progress indicators do not always accurately represent the status of the backup/restore process.
ISPROD-14367 | When labeling in the ViDi EL Segment tool, if the first trained image has no labels applied, the ViDi EL Segment tool does not produce any results regardless of any further labeling on subsequent training images.
ISPROD-15217 | Several tools have regions out of bounds and cannot be added.
ISPROD-15691 | When the EL Segment tool is trained on one platform, a device or an emulator, it gives different results on the other platform.
ISPROD-15724 | The EditBounds regions do not update when the image changes.
ISPROD-16124 | Selecting a directory in Save Job does not save.
ISPROD-16747 | The Online/Offline event does not run when the system goes offline since the TaskQueue is cleared when going offline.
ISPROD-16828 | Ethernet IP over USB-C link local support does not exist for all In-Sight 3800 models.
ISPROD-18131 | Password encrypted by EditPassword tool is displayed in the property sheet as plain text on D900.
ISPROD-19115 | WebHMI memory leaks cause In-Sight vision systems to stop responding
ISPROD-17634 | Japanese characters do not display correctly in the Web HMI.
ISPROD-16192 | In-Sight adapters do not display properly after changing display resolution. Disconnecting and reconnecting to the vision system fixes the issue.
ISPROD-21390 | The Count Blob tool is missing in the EasyBuilder for In-Sight 2800M-EC vision systems that were shipped with firmware earlier than In-Sight 22.3.0.
ISPROD-20896 | Encoder lines for line scan vision systems are not configurable in the GUI.
ISPROD-20790 | When scheduling multiple triggers, the elapsed time for the first trigger is approximately twice as long as the subsequent triggers.
ISPROD-20349 | The WriteImage function fails to save PlotString output correctly using the SVG Overlay or Render on Image settings.
ISPROD-18933 | The SetOnline Native Mode command returns a success message when issued while the operator is forcing the vision system offline.
ISPROD-17738 | EL tools cannot be trained after removing and re-applying a license. Workaround: restart In-Sight Vision Suite.
ISPROD-21389 | Users cannot access the File Management utility with SSO credentials if the password contains a special character such as @ or ^.