# SetWhiteBalanceGain

Available for color In-Sight L38 series vision systems only, the SetWhiteBalanceGain function Functions are tools that are available in Spreadsheet for processing and analyzing acquisitions or other results. You can add functions to your Spreadsheet job to create tool chains and produce results for specific applications. is used to configure the gain value of the specified color channel (red, green, or blue) in a white balanced image.

Note: The SetWhiteBalanceGain function is not listed in the . To open its Property Sheet and configure it, type SetWhiteBalanceGain() into a Spreadsheet cell.

## SetWhiteBalanceGain Inputs

The SetWhiteBalanceGain function has the following parameters listed in its Property Sheet.

Parameter | Description
--- | ---
Color Channel | Specifies the color channel whose gain value will be set: Red = 0 Green = 1 Blue = 2
Gain Value | Specifies the gain value to set for the channel specified with the Color Channel parameter. The value is a float, with a range of 1 to 255. The default value is 1.

### SetWhiteBalanceGain Outputs

Parameter | Description
--- | ---
Returns | A ❒SetWhiteBalanceGain structure, containing the configured gain value of the specified color channel. Double-click the structure to open the tool's Property Sheet again.

### SetWhiteBalanceGain Vision Data Access functions

The SetWhiteBalanceGain tool has no specific Vision Data Access functions.