# Point

Creates a fixtured Point structure.

Inputs

Parameter | Description
Image | This argument must reference a spreadsheet cell that contains a valid Image data structure. By default, the cell referenced is cell A1, containing the Image data structure .
Fixture A fixture is a coordinate location on the image that keeps the tool in the place determined by the fixture. | Specifies the image coordinate system in which the point is defined.
X | The X-offset of the fixture.
Y | The Y-offset of the fixture.
Theta | The rotation from the image X-axis, in the image coordinate system. (+/-360 degrees clockwise)
Point | Specifies the location of the point, in fixture coordinates.
X | The X-coordinate of the point.
Y | The Y-coordinate of the point.
Show | Specifies the display mode for the Point overlay graphic on the image.
0 = hide all (default) | The point structure is hidden unless the cell containing the Point function Functions are tools that are available in Spreadsheet for processing and analyzing acquisitions or other results. You can add functions to your Spreadsheet job to create tool chains and produce results for specific applications. is highlighted in the spreadsheet.
2 = input graphics only | The point structure is always displayed.

Note: The Fixture and Point parameters must be defined within the bounds of the image. Otherwise, the function returns #ERR.
Outputs

Returns | A Point data structure, or #ERR if any of the input parameters are invalid.
Results | When Point is initially inserted into a cell, the following Structures Vision Data Access functions are automatically inserted into the spreadsheet to create the result table:
Label | Function | Description
X | GetX(Point) | Returns an X-coordinate of the point.
Y | GetY(Point) | Returns an Y-coordinate of the point.