# In-Sight 3800 Utilities

Utility Button | Utility Name | Description | Minimum User Access Level
--- | --- | --- | ---
| Firmware Update | The Firmware Update utility helps you through the firmware update process. For more information, see Firmware Update. | Full
| Restart | The Restart utility remotely restarts an In-Sight vision system. For more information, see Restart. | Elevated
| Backup | The Backup utility backs up the selected vision system(s). For more information, see Backup. | Elevated
| Restore | The Restore utility restores the selected In-Sight vision system. For more information, see Restore. | Full
| User Settings | The User Settings utility allows you to configure users and their access capabilities on an In-Sight vision system. For more information, see User Settings. | Full
| Industrial Ethernet | The Industrial Ethernet utility selects and configures an Industrial Communications protocol for the vision system. For more information, see Industrial Ethernet. | Elevated
| Camera Configuration | The Camera Configuration utility allows you to configure the resolution for the vision system. For more information, see Camera Configuration. | Elevated
| Go Offline | The Go Offline utility sets an Online job Offline on an In-Sight vision system. For more information, see Go Offline. | Elevated
| File Management | The File Management utility allows you to view, copy, move, or delete files on the In-Sight vision system. For more information, see File Management. | Elevated
| Startup Settings | The Startup Settings utility configures a startup job for the In-Sight vision system. For more information, see Startup Settings. | Elevated
| License Configuration | The License Configuration utility updates the existing product license of your In-Sight vision system on the Cognex Security Dongle. For more information, see License Configuration. | Full
| Network Settings | The Network Settings utility configures the network settings of an In-Sight vision system. For more information, see Network Settings. | Elevated
| Time Settings | The Time Settings utility is used to configure the date and time settings of an In-Sight vision system. For more information, see Time Settings. | Elevated
| Password Reset | The Password Reset utility resets the password of the default admin user on the selected In-Sight vision system(s). For more information, see Password Reset. | None
| Factory Reset | The Factory Reset utility restores an In-Sight vision system to its factory default settings. For more information, see Factory Reset. | Full
| HMI Settings | The HMI Settings utility allows you to configure the HMI window. For more information, see HMI Settings. | Elevated
| Audit Logging | The Audit Logging utility allows you to create audit logs, download the log, or forward the log to a remote server. For more information, see Audit Logging. | Full
| System Validation | The System Validation utility allows you to verify the current state of the vision system and configure system changes that can invalidate it. For more information, see System Validation. | Full
| Calibration Grid | The Calibration Grid utility prints out a calibration grid paper to assist in calibrating between pixel and real-world coordinates. For more information, see Calibration Grid. | None
| Support Feedback | The Support Feedback utility (also known as the Report a Problem utility) prepares error reports for potential issues. For more information, see Support Feedback. | Elevated
| Serial Configuration | The Serial Configuration utility allows you to configure the serial port of the vision system. For more information, see Serial Configuration. | Elevated
| Configure SMB | The Configure SMB utility configures the Server Message Block (SMB) protocol settings of your In-Sight vision system. For more information, see Configure SMB. | Elevated
| IP Licensing | The IP Licensing utility adds job licenses to your In-Sight vision system. For more information, see IP Licensing. | Full
| Secure Connection | The Secure Connection utility allows you to encrypt HMI communications. For more information, see Secure Connection. | Full