# Resolved Issues

This section describes changes and resolved issues in In-Sight EasyBuilder 25.2.0.

Note: Issue numbers (Issue #) have been included (where applicable) to improve tracking of Known Issues reported via Cognex Technical Support.

##### Resolved Issues in In-Sight EasyBuilder 25.2.0

Issue # | Resolved Issue
--- | ---
ISPROD-19556 | OPC UA tags are now added even if the cells contain an #ERR.
ISPROD-21410 | Fixed an issue where the GUI of ViDiELClassify could sporadically crash when assigning labels while the tool was in the process of training.
ISPROD-22187 | Fixed an issue where the wrong image format would be displayed in the dropdown of the filmstrip after restarting In-Sight EasyBuilder.
ISPROD-23254 | Startup Settings utility now has an FTP fallback mode.
ISPROD-23257 | Fixed an issue where images would be saved in .bmp format despite selecting .jpg in the Save Image As window.
ISPROD-23864 | Fixed an issue where switching between the Image and Inspect application steps could cause a memory leak.
ISPROD-23959 | Fixed an issue where the vision system could not be assigned a static IP address when upgrading to 25.1.0.
ISPROD-24137 | Fixed an issue where the system could not accept new triggers when running out of image buffers until restart.
ISPROD-24257 | Fixed an issue where Edge Learning Edge Learning is an AI-based technology used for inspections and other judgement-based tasks, to help improve quality control and optimize efficiency. The training also happens on the vision system without any external graphical accelerator. tools could sporadically cause memory corruption and fail with color images.
ISPROD-24398 | Fixed an issue where Edge Learning tools could fail with the following error message: "Error. Invalid combination of color planes".