# Importing the GSD File into the Catalog

The In-Sight vision system appears in the Catalog only if its GSD file is installed. This must be performed only once, when the vision system is configured on the PLC the first time.

To install the GSD file for the In-Sight vision system, follow the below steps:

1. Click on the Options menu, and then on the Install general station description file (GSD) option.

2. Browse the folder containing the GSD file:

3. Tick the box in front of the GSDML file, then click on Install.