# In-Sight System Requirements

Note: The following minimum hardware requirements are for PCs that are connected to a single low-resolution (1 MP) In-Sight vision system running at a slow production speed.

Name | Minimum Requirement | Standard Requirement
--- | --- | ---
Disk Space | 4 GB | 20 GB SSD
RAM | 8 GB | 8 GB
Network Speed | 100 Mb/s | 1000 Mb/s
USB Port | USB 2.0 | USB 2.0
Processor | Intel Celeron J1900 or AMD A6-5200 | i3-6100 (or better) and AMD Ryzen 3 1200 (or better)
Display Resolution | 1024x640 1366x768 1920x1080 | 1920x1080