# Resolved Issues

This section describes changes and resolved issues in In-Sight 23.1.1 and past releases.

Note: Issue numbers (Issue #) have been included (where applicable) to improve tracking of Known Issues reported via Cognex Technical Support.

##### Resolved Issues in In-Sight 23.1.1

Issue # | Resolved Issue
IS280-10672 | Record/Playback performance declines with large (100+) numbers of images. As the image count grows to hundreds, scrolling images becomes slow.
ISPROD-1355 | Self-trigger mode does not overlap acquisition when the job execution exceeds the trigger interval. Instead, the next acquisition is simply delayed until the job execution is complete. This means that for long-running jobs, the self-trigger interval is determined by whichever is longer.
ISPROD-5069 | The SW8 Native Mode Command responds before the inspection is complete.
ISPROD-6400 | The WriteData with Append option fails to perform as expected due to parallel transfers causing interleaved writes.
ISPROD-6900 | The In-Sight goes into a bad state. It needs to be rebooted if the partial acquisition settings are modified immediately after taking the In-Sight offline.
ISPROD-6938 | Emulator shows EL tools even when a cloud or physical dongle is not present. Attempting to add one of these tools without the dongle results in an error message.
N/A | If you want to remove the InSightEmulator dongle but the remove button is grayed out, use one of the following solutions: When you install the CodeMeter SDK, the remove button is enabled. When you install the CodeMeter Runtime the remove button is disabled. There is a registry key: Computer\HKEY_CURRENT_USER\Software\WIBU-SYSTEMS\CodeMeterCC Setting the value of AllowCmActDelete to 1 enables the button. This is a feature from WiBu to prevent customers from accidentally deleting licenses.
ISPROD-6536 | If your network drops or if you remove the cloud dongle while emulating and using EL tools, licensing errors appear and cause the emulator to crash.
ISPROD-6216 | When triggering the camera from a PLC, the TriggerReady signal malfunctions and stays low even when the trigger is ready. When in this state, the PLC can still trigger the camera.
ISPROD-2306 | Filmstrip and Record/Playback performance declined with large (100+) numbers of images. As the image count grew to the hundreds, images scrolled slowly. It now handles a lot more images.
ISPROD-118 | The Math tool was unable to link to the fixture from a Pattern tool.
ISPROD-127 | In some circumstances, the Classify tool would fail to show unlabeled images for training after they were unlabeled.
ISPROD-539 | The EditPolygon tool did not allow removing points through the right click context menu.
ISPROD-1703 | Rename EasyView item when cell is renamed.
ISPROD-1770 | ClearResultBuffer does not clear the results (in the PLC) and #ERRs when executing.
ISPROD-5866 | The installer does not run because of NullReferenceException.
ISPROD-6216 | When triggering the camera from a PLC, the TriggerReady signal could get in a state where it stays low even when the trigger is ready.
ISPROD-6654 | The FTP file path was incorrectly appending itself to the filename when writing data to the FTP server.
ISPROD-6771 | GetAngle on a ReadIDMax returned incorrect angles.
ISPROD-6939 | Registry Editor keeps showing up after registering the emulator.
ISPROD-6941 | ImageBuffer shrinks when over-triggering.
ISPROD-6986 | SFTP transfers attempted to write to the SFTP servers root directory, not the SFTP home directory. This can be re-enabled by setting the directory to "/".
ISPROD-6988 | Exposure end event is delayed. (Fixed on 3800 models only.)
ISPROD-7044 | Triggering while online and then going offline and enabling HDR caused the In-Sight to become unresponsive.
ISPROD-7046 | Rapid triggering could result in out-of-focus HSLL.
ISPROD-7133 | HMI Edit Graphics not working after triggering.
ISPROD-7180 | Changing the Verify Partial Acq settings after going offline stops image acquisition.
ISPROD-7157 | 2805M should not have white-balance enabled.
ISPROD-7248 | If HDR+ is toggled on a color device, sometimes acquisiton will lock up.
ISPROD-7312 | Can only start the oldest emulator even with multiple adapters installed.
ISPROD-7371 | Getting the field-diagnostics archive from In-Sight often does not work, especially when something goes wrong.
ISPROD-7617 | The Job Converter failed to import any spreadsheet function with an angle as a function parameter.
ISPROD-7627 | Focus Position adjustment does not work when pulled into the spreadsheet.
ISPROD-7765 | Acquisition stops after autoexposure.
ISPROD-8002 | Font size does not change until trigger.
ISPROD-8004 | Spreadsheet cell width is not shown correctly when a new job is loaded.
ISPROD-8034 | Logistics detector loses defaults.
ISPROD-8758 | Jobs incorrectly converted when the GUI language was not English.
ISPROD-9112 | Moving added regions in the EditCompositeRegion property sheet crashes the SS/GUI.
ISPROD-9024 | Inconsistent behavior when changing the Focus Position using ApplyAcquisitionSettings online.
ISPROD-9084 | Emulator starts with no sensors on network.