# Get Online

Returns the Online state of theVision System.

## Get Online Inputs

Syntax: GO

## Get Online Outputs

Returns the Online state of the vision system.

Online State | Description
--- | ---
0 | The Vision System is currently Offline.
1 | The Vision System is currently Online.

## Get Online Example

To determine the Online state of the Vision System, issue the following command: GO

The Vision System responds with 1, indicating that the vision system is currently Online.