# Resolved Issues

This section describes changes and resolved issues in In-Sight 23.3.0.

Note: Issue numbers (Issue #) have been included (where applicable) to improve tracking of Known Issues reported via Cognex Technical Support.

##### Resolved Issues in In-Sight 23.3.0

Issue # | Resolved Issue
ISPROD-971 | Fixed a delayed response when working on a job with lots of cells.
ISPROD-4320 | Fixed the issue when SVGs and images with graphics are clipped incorrectly if browser scaling is enabled.
ISPROD-6133 | Added a console window to aid Script development.
ISPROD-6595 | Fixed the issue when the License Configuration utilities do not prompt for authentication.
ISPROD-6962 | The Job Status settings and the Custom View settings are not disabled when online or live mode.
ISPROD-7268 | Fixed an issue preventing the deletion of jobs or files whose file names have certain special characters, such as #.
ISPROD-7301 | Fixed the circular reference after adding a job property link in Math Tool.
ISPROD-7578 | Fixed the issue when the camera connection crashes after resetting the acquisition settings.
ISPROD-7907 | Fixed the issue where Pixel Count results were not consistent enough for certain regions or shapes.
ISPROD-8431 | Avoiding the Windows 11 Clipboard "Suggested Actions" feature via software.
ISPROD-8482 | Fixed the default white balance discoloration for IS 3800 devices.
ISPROD-9159 | Fixed the problems with the License Dialog when the admin password is not the default.
ISPROD-9308 | Fixed the issue that the GetSetCodeType Spreadsheet function crashes the emulator.
ISPROD-11650 | The imported calibration data that contains more than four points can now be used as TransPixelToWorld input.
ISPROD-7246 | OCRMax, ExtractCalibrationPoints, and Script functions now return a checksum/dataID when queried using the Web API HmiSession::getCellExpressions request.
ISPROD-11133 | The device list in In-Sight Vision Suite no longer cuts off details when the device list is expanded and the devices are shown in card view.
ISPROD-12790 | Serial configuration can now be configured for Text (default) or Native to accept native mode commands.
ISPROD-12283 | The ReadSerial and WriteSerial functions now handle values larger than 0x7F by user preference. This enables backwards compatibility with In-Sight Explorer. WriteSerial now has a parameter to send raw data (checked by default) or UTF-8 encoded data (unchecked).
ISPROD-11827 | Native mode command SS no longer adds an extra 0 character when using the expected cell name format.
ISPROD-11669 | Improved performance when disabled trigger modes prevent pre-armed acquisitions. The vision system no longer fires and processes additional missed acquisition event.
ISPROD-9674 | The IO defaults of Advantage 182 do not show OUT0 as bi-directional.
ISPROD-12858 | The EasyBuilder WriteImage function cannot add timestamp to name when set by industrial protocol.
ISPROD-11448 | WebHMI overwrites the ListBox value when a trigger occurs.
ISPROD-11003 | A few WebHMI graphics do not match graphics in In-Sight Vision Suite.
ISPROD-11377 | Auto UI Reconnects can start to fail after two consecutive reconnects.
ISPROD-10336 | In OCRMax, characters labeled with a '?' do not appear on the tree view.
ISPROD-12823 | The Read ID tool in EasyBuilder now fails when no barcodes are detected.
ISPROD-9296 | OCRMax cell supported as a type in ImportData and ExportData.
ISPROD-11886 | Added Training option to Read ID tool in EasyBuilder.
ISPROD-12060 | Added Verify checkbox to ReadIDMax tool and associated vision data access functions in Spreadsheet.
ISPROD-218 | Added a toolbar button to save the current image in EasyBuilder.
ISPROD-10249 | Removed persistent pink highlighting around changed cells when displaying cell dependencies.
ISPROD-12585 | Changed the In-Sight Vision Suite TCP client minimum timeout to 100 ms from 1000 ms to match In-Sight Explorer.
ISPROD-12812 | Fixed the issue where jobs with the DetectBlobs tool can cause the vision system to reboot when using a composite polygon input region.
N/A | ViDi EL Read has been improved to prevent misclassifying characters, especially when fielding is used, and improved character scoring.
N/A | The run-time performance of the ViDi EL Classify and ViDi EL Read tools has been improved. Jobs with ViDi EL tools that were created prior to 23.3.0 will take longer to execute while the tools undergo the initial retraining process. After the initial retraining, job load times will return to normal.