# ApplyAcquisitionSettings Vision Data Access Functions

This section lists the available 3D Vision Data Access Functions that get values from the vision system ApplyAcquisitionSettings function.

Note: Each of the following functions references an ApplyAcquisitionSettings structure for the first parameter. Index (zero-based) determines which acquisition of the ApplyAcquisitionSettings structure you want to reference. If you do not specify the index, the index defaults to zero, meaning the function returns the first acquisition.

Function | Description
GetDetectionZoneZMax(ApplyAcquisitionSettings, [Index]) | Returns the Detection Zone Z Max value defined by the ApplyAcquisitionSettings function.
GetDetectionZoneZMin(ApplyAcquisitionSettings, [Index]) | Returns the Detection Zone Z Min value defined by the ApplyAcquisitionSettings function.
GetExposure(ApplyAcquisitionSettings, [Index]) | Returns the Exposure value defined by the ApplyAcquisitionSettings function.
GetGenerate2DGrey(ApplyAcquisitionSettings, [Index]) | Returns the Generate 2D Grey value defined by the ApplyAcquisitionSettings function.
GetSensitivity(ApplyAcquisitionSettings, [Index]) | Returns the Sensitivity value defined by the ApplyAcquisitionSettings function.
GetYResolution(ApplyAcquisitionSettings, [Index]) | Returns the Y Resolution value defined by the ApplyAcquisitionSettings function.