# Filmstrip Files

Each frame of the Filmstrip is stored as a set of image and data files in the folder specified with the (Configure the Record and Playback Directory) button, or in the ZIP file created with the Save Images buttons. Each Filmstrip frame consists of the following files:

- *.cfg: The frame configuration file, containing information on the frame's JSON data file, the vision system model, the name of the job, and the date/time when the frame was recorded. The name of the *.cfg file is identical to the frame name shown in the Filmstrip (that is, if a frame is renamed in the Filmstrip window, then its configuration file is also renamed).

  Note: Do not edit the contents of the *.cfg files directly through a text editor.
- *.dat: The data file of the 3D point cloud. Each frame has two data files, containing the basic and high-resolution point cloud data, respectively (the latter having a _HighRes suffix).
- *.json: The data file of the frame, containing acquisition information and defining the *.dat and *.raw files of the frame.
- *.png: The thumbnail image of the constructed point cloud used on the Filmstrip. This file always has a _Thumb suffix in its name.
- *.raw: The recorded raw image file of the acquisition.

Note:

Hover the cursor over a frame to display its detailed information, including the frame's configuration file name and location, the date and time of recording, and the name of the job in which the frame was created.