# In-Sight 3D-L4000 Series I/O Lines

## Number of Input and Output Lines

In-Sight Vision System | Direct Inputs | Direct Outputs
In-Sight 3D-L4000 Series | 1 acquisition trigger input | Up to 2 high-speed outputs 1 user-configurable LED (1 green or red, 1 red)

## Input and Output Lines

In | Out | Direction | Name
0 |  | Fixed Input | TRIGGER
| 0 | Fixed Output | HSOUT 0
| 1 | Fixed Output | HSOUT 1
| 2 | Fixed Output | Pass/Fail LED

Note: TRIGGER is reserved for acquisition trigger input and cannot be configured.