# GetBufferData

Returns the indexed data from a ReadEIP, ReadProfinet, ReadDeviceNet, or ReadModbus structure.

Note: GetBufferData does not have a property sheet. You can configure this function directly in the cell, or in the Formula Bar on the Job Edit toolbar, either by typing in cell values directly, or selecting the cell references of the supported data structures.

## GetBufferData Inputs

Parameter | Description
--- | ---
Data Structure | ReadEIP, ReadProfinet, ReadDeviceNet, Readmodbus data structure.

## GetBufferData Outputs

Returns | ReadEIP, ReadProfinet, ReadDeviceNet, ReadModbus indexed data.