# Create an HMI for Operators

WebPages allow you to create a Web browser-based Human Machine Interface (HMI) for operators to interact with the job while the In-Sight vision system is online.

By default, the In-Sight ViDi adapter has two preconfigured WebPages to help you setup and configure your job.

Note: The Web Page Editor is open by default. In case it is closed, select View > Web Pages. For more information, see Display the WebPage Editor.

Main
| This WebPage contains the following: A Display element which shows the image being processed by the spreadsheet in the AcquireImage cell. A Button element configured to trigger an acquisition (Button Click Command Property set to Tasks.InspectionTask.Run). A Button element configured to launch the Cam0Setup WebPage (Click Command property set to HMI.ShowPage). A Filmstrip element configured to interact with the Filmstrip. A Run-Pause element, which toggles the state of the $RunEnableHMI tag (refer to the Pause While Online topic for more information).

Cam0Setup
| This WebPage contains the following: A Live Display element which displays the image directly acquired from the vision system. A set of Numeric Entry elements set to the Delay, Exposure, Offset and Gain properties of the vision system. A Run-Pause element, which toggles the state of the $RunEnableHMI tag (refer to the Pause While Online topic for more information).

After you have created your job logic in the Spreadsheet Editor, you can either select a group of cells (Create a WebPage from Selected Cells) and create a new WebPage from them, or select individual cells and generate Tags (Publish) and then drag and drop them onto a WebPage (Drag-and-Drop Tags to Web Pages).