# Job Execution, Acquisition Trigger Mode and Related Events Timing Diagrams

The following timing diagrams provide illustrations of sample job execution, acquisition and events related to the two:

- Continuous Trigger Mode

- Continuous Trigger Mode with Delay (ms)

- Camera or Industrial Ethernet Trigger Modes

- Camera or Industrial Ethernet Trigger Modes with Delay (ms)

- Acquisition Missed

- Discrete Output Signals

  Note: The Acquire End signal occurs partway through the Acquisition cycle, at the end of the Exposure period, and prior to transferring the acquired image into memory to be processed by the Spreadsheet.