# Modify Acquisition Settings with ApplyAcquisitionSettings

The ApplyAcquisitionSettings function allows you to adjust the parameters of the AcquireImage from the spreadsheet, and by extension, the Web HMI. When the ApplyAcquisitionSettings function is executed, it modifies the specified acquisition settings in AcquireImage, and overrides the values specified in AcquireImage.

The ApplyAcquisitionSettings function only executes when one of its input arguments changes, or when forced to execute via a conditional cell state becoming enabled.

Note: Please refer to the ApplyAcquisitionSettings function topic for information about parameters and their settings. This topic is meant as an introduction to the function.