# Importing the GSD File into the Catalog

The In-Sight vision system appears in the Catalog only if its GSD file is installed. This must be performed only once, when the vision system is configured on the PLC the first time.

To install the GSD file for the vision system, follow the below steps:

1. Click on the Options menu, and then on the Install GSD File option.

2. Browse the folder containing the GSD file, as shown below. By default, it is in the following directory:

   C:\Program Files\Cognex\In-Sight\In-Sight Vision Suite Adapters\In-Sight ViDi 1.2.0\FFP\In-Sight D9xx\GSD

3. Press the Select All button, then click on Install.