# Resolved Issues

This section describes changes and resolved issues in In-Sight 3D EasyBuilder 25.3.0.

Note: Issue numbers (Issue #) have been included (where applicable) to improve tracking of Known Issues reported via Cognex Technical Support.

##### Resolved Issues in In-Sight 3D EasyBuilder 25.3.0

Issue # | Resolved Issue
--- | ---
ISPROD-22951 | Fixed an issue where the Min and Mean functions produced inconsistent results when processing cell ranges that include cells with #ERR.
ISPROD-22190 | Fixed an issue when using the TrainExtractColor function Functions are tools that are available in Spreadsheet for processing and analyzing acquisitions or other results. You can add functions to your Spreadsheet job to create tool chains and produce results for specific applications., masked images did not display overlapping ColorGroups correctly.
ISPROD-26410 | WebHMI The operator interface through which the operator interacts with the vision system. auto saving of 3D visualization settings is readded.
ISPROD-26300 | Fixed an issue for In-Sight L38 vision systems where the acquisition Acquisition is the process or result of the vision system acquiring a new image. timeout was sometimes not applied after the third acquisition.
ISPROD-26187 | Fixed an issue where uninstalling In-Sight Vision Suite 25.3.0 lead to device discovery not working with older versions of In-Sight Vision Suite.
ISPROD-25878 | Fixed an issue where it was impossible to set certain SLMP server addresses.
ISPROD-25760 | The ROI of the Classify tool is now fixed after the image is trained.
ISPROD-25575 | Fixed an issue where Native Mode commands caused Telnet connection to close.
ISPROD-25481 | Fixed an issue where the user field in the audit logs was inconsistent.
ISPROD-25347 | Fixed time delay reference for digital outputs.
ISPROD-25330 | Fixed an issue where it was possible to trigger the vision system through FFP acquire command when the vision system was offline.
ISPROD-25276 | Fixed an issue where the acquisition for the In-Sight 2800 vision system would lock up at high exposure values.
ISPROD-25170 | Fixed an issue where the maximum allowed value for a line scan emulator was lower than an actual line scan vision systems.
ISPROD-25023 | Fixed an issue where the Calibration Grid utility could print a target with wrong dimensions.
ISPROD-23516 | Fixed an issue where creating more than one ViDiELSegment tool with high resolution and small feature size could crash Performance and Max vision system models.
ISPROD-24590 | Fixed an issue with the ViDiELClassify3D tool displaying one of the already trained images in the Train tab after training.
ISPROD-25504 | Increased the number of elements in the FormatInputBuffer to more than 128.